// ----------------------------------
// RSDK Project: Sonic 1/Sonic 2
// Script Description: Belt Platform Object
// Script Author: Christan Whitehead/Simon Thomley
// Unpacked by Rubberduckycooly's script unpacker
// ----------------------------------

//-------Aliases-------//
private alias 65 : TYPE_BELTPLATFORM

// Function declarations
reserve function BeltPlatform_Function151

// Static Values

// Tables
public table BeltPlatform_table35
	10, 8, 6, 6, 8, 6
end table

public table BeltPlatform_table34
	0, 0, 0, 0, 0, 0
end table

private table BeltPlatform_table0
	0x1078, 538, 0x10BE, 608, 0x10BE, 915, 0x108C, 965, 0x1022, 912, 0x1022, 580
end table

private table BeltPlatform_table1
	0x127E, 640, 0x12CE, 720, 0x12CE, 0x46E, 0x1232, 0x420, 0x1232, 716
end table

private table BeltPlatform_table2
	0xD22, 0x482, 0xD22, 0x5DE, 0xDAE, 0x5DE, 0xDAE, 0x482
end table

private table BeltPlatform_table3
	0xD62, 930, 0xDEE, 930, 0xDEE, 0x4DE, 0xD62, 0x4DE
end table

private table BeltPlatform_table4
	0xCAC, 578, 0xDDE, 578, 0xDDE, 990, 0xC52, 990, 0xC52, 668
end table

private table BeltPlatform_table5
	0x1252, 522, 0x13DE, 522, 0x13DE, 702, 0x1252, 702
end table

function BeltPlatform_Function151
	temp0 = object[arrayPos0].value5
	GetTableValue(object[arrayPos0].value0, temp0, object[arrayPos0].value4)
	temp0++
	GetTableValue(object[arrayPos0].value1, temp0, object[arrayPos0].value4)
	temp0 = object[arrayPos0].ixpos
	temp0 -= object[arrayPos0].value0
	Abs(temp0)
	temp1 = object[arrayPos0].iypos
	temp1 -= object[arrayPos0].value1
	Abs(temp1)
	if temp1 < temp0
		object[arrayPos0].xvel = 0x10000
		temp1 <<= 16
		object[arrayPos0].yvel = temp1
		object[arrayPos0].yvel /= temp0
	else
		if temp1 != 0
			temp0 <<= 16
			object[arrayPos0].xvel = temp0
			object[arrayPos0].xvel /= temp1
		else
			object[arrayPos0].xvel = 0
		end if
		object[arrayPos0].yvel = 0x10000
	end if
	if object[arrayPos0].value0 < object[arrayPos0].ixpos
		FlipSign(object[arrayPos0].xvel)
	end if
	if object[arrayPos0].value1 < object[arrayPos0].iypos
		FlipSign(object[arrayPos0].yvel)
	end if
end function


event ObjectMain
	temp2 = 0
	if object.value7 != LZSetup_value30
		object.direction ^= FLIP_X
		object.value7 = LZSetup_value30
		temp2 = 1
	else
		temp0 = object.xpos
		temp1 = object.ypos
		temp0 >>= 16
		temp1 >>= 16
		if temp0 == object.value0
			if temp1 == object.value1
				temp2 = 1
			end if
		end if
	end if
	if temp2 == 1
		if object.direction == FLIP_NONE
			object.value5 += 2
			if object.value5 > object.value6
				object.value5 = 0
			end if
		else
			object.value5 -= 2
			if object.value5 < 0
				object.value5 = object.value6
			end if
		end if
		arrayPos0 = object.entityPos
		CallFunction(BeltPlatform_Function151)
	end if
	temp0 = object.xpos
	temp0 &= -0x10000
	temp1 = object.ypos
	temp1 &= -0x10000
	temp2 = object.xpos
	temp2 += object.xvel
	temp3 = object.ypos
	temp3 += object.yvel
	object.value2 = temp2
	object.value2 &= -0x10000
	object.value2 -= temp0
	object.value3 = temp3
	object.value3 &= -0x10000
	object.value3 -= temp1
	foreach (GROUP_PLAYERS, currentPlayer, ACTIVE_ENTITIES)
		BoxCollisionTest(C_PLATFORM, object.entityPos, -16, -8, 16, 8, currentPlayer, HITBOX_AUTO, HITBOX_AUTO, HITBOX_AUTO, HITBOX_AUTO)
		if checkResult == 1
			object[currentPlayer].xpos += object.value2
			object[currentPlayer].ypos += object.value3
		end if
	next
	object.xpos = temp2
	object.ypos = temp3
end event


event ObjectDraw
	DrawSprite(0)
end event


event ObjectStartup
	LoadSpriteSheet("LZ/Objects.gif")
	SpriteFrame(-16, -8, 32, 16, 223, 154)
	SetTableValue(BeltPlatform_table0, 0, BeltPlatform_table34)
	SetTableValue(BeltPlatform_table1, 1, BeltPlatform_table34)
	SetTableValue(BeltPlatform_table2, 2, BeltPlatform_table34)
	SetTableValue(BeltPlatform_table3, 3, BeltPlatform_table34)
	SetTableValue(BeltPlatform_table4, 4, BeltPlatform_table34)
	SetTableValue(BeltPlatform_table5, 5, BeltPlatform_table34)
	foreach (TypeName[Belt Platform], arrayPos0, ALL_ENTITIES)
		object[arrayPos0].priority = PRIORITY_INACTIVE
		temp0 = object[arrayPos0].propertyValue
		temp0 >>= 4
		GetTableValue(object[arrayPos0].value4, temp0, BeltPlatform_table34)
		GetTableValue(object[arrayPos0].value6, temp0, BeltPlatform_table35)
		object[arrayPos0].value5 = object[arrayPos0].propertyValue
		object[arrayPos0].value5 &= 15
		object[arrayPos0].value5 <<= 1
		CallFunction(BeltPlatform_Function151)
	next
end event

event RSDKDraw
	DrawSprite(0)
end event

event RSDKLoad
	LoadSpriteSheet("Global/Display.gif")
	SpriteFrame(-16, -16, 32, 32, 1, 143)
end event
